NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Kenya **If applicable, name of local government involved (Article 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** Kenya Bureau of Standards**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:** P.O. Box: 54974-00200, Nairobi, KenyaTelephone: + (254) 020 605490, 605506/6948258Fax: + (254) 020 609660/609665E-mail: info@kebs.org; Website: <http://www.kebs.org> |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****X],** **5.7.1 [****],** **other****:**  |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Doors and their frames and thresholds, of wood (HS 441820); Doors and windows (ICS 91.060.50) |
| **5.** | **Title, number of pages and language(s) of the notified document:** DEAS 1067:2021, General wooden door shutters — Specification, First Edition (30 page(s), in English) |
| **6.** | **Description of content:** This Draft East Africa Standard specifies requirements, sampling and test methods for wooden door shutters of three exposure classes and three performance classes. This specification does not cover the requirements for fire doors. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Consumer information, labelling; Prevention of deceptive practices and consumer protection; Quality requirements; Harmonization; Reducing trade barriers and facilitating trade |
| **8.** | **Relevant documents:** 1. ISO 6445, Doors -- Behaviour between two different climates -- Test method
2. ISO 7894, Partitions made of components -- Test for resistance to wind (static pressure and slamming doors
3. ISO 8270, Door sets — Soft heavy body impact test
4. ISO 12777-3, Methods of test for pallet joints -- Part 3: Determination of strength of pallet joints
5. EAS 272, Timber — Determination of moisture content for physical and mechanical tests
6. ISO 6443, Door leaves — Method for measurement of height, width, thickness and Squareness
7. ISO 8271, Door leaves — Determination of the resistance to hard body impact
8. ISO 9380, Door sets — Repeated torsion test
9. US 1777: 2017, General wooden door shutters — Specification
 |
| **9.** | **Proposed date of adoption:** To be determined**Proposed date of entry into force:** To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:** Kenya Bureau of StandardsWTO/TBT National Enquiry PointP.O. Box: 54974-00200, Nairobi, KenyaTelephone: + (254) 020 605490, 605506/6948258Fax: + (254) 020 609660/609665E-mail: info@kebs.org; Website: <http://www.kebs.org><https://members.wto.org/crnattachments/2021/TBT/KEN/21_7800_00_e.pdf> |