NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** BOTSWANA**If applicable, name of local government involved (Article 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** BOTSWANA BUREAU OF STANDARDSPrivate Bag B0 48Gaborone,Botswana.Tel : (+267) 3903200Fax:(+267)3903120Toll Free Number : (0800 600 900)E-mail : infoc@hq.bobstandards.bw**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:**  |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****],** **5.7.1 [****], 3.2 [****], 7.2 [****],** **other****:**  |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Lighting, signalling and warning devices (ICS code(s): 43.040.20) |
| **5.** | **Title, number of pages and language(s) of the notified document:** BOS 320:2009 Retro-reflectors (Reflex reflectors) - Specification; (17 page(s), in English) |
| **6.** | **Description of content:** This specification covers the requirements for sealed red, amber and clear (white) retro-reflectors (reflex reflectors) for use on road vehicles, including retro-reflectors that form part of light assemblies.This specification does not cover1. flexible retro-reflective material;
2. retro-reflective warning signs; or
3. retro-reflective registration plates.

NOTE 1 Information that must be supplied by the test sponsor is given in Annex A.NOTE 2 Information regarding the verification of the quality of retro-reflectors produced to this specification, and the sampling plan to be used to assess compliance with the specification of a lot of retro-reflectors are given in Annex B. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** National security requirements; Protection of human health or safety |
| **8.** | **Relevant documents:** BOS ISO 2859-1 *Sampling procedures for inspection by attributes – Part 1: Sampling schemes indexed by acceptance quality level (AQL) for lot-by-lot inspection.*BOS ISO 9001, *Quality management systems – Requirements.*ISO 9227, *Corrosion tests in artificial atmospheres – Salt spray tests.* |
| **9.** | **Proposed date of adoption:** To be determined**Proposed date of entry into force:** To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:** BOTSWANA BUREAU OF STANDARDSPrivate Bag B0 48Gaborone,Botswana.Tel : (+267) 3903200Fax:(+267)3903120Toll Free Number : (0800 600 900)E-mail : infoc@hq.bobstandards.bw |