NOTIFICATION

The following notification is being circulated in accordance with Article 10.6.

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** CHILE**If applicable, name of local government involved (Articles 3.2 and 7.2):** |
| **2.** | **Agency responsible:***Dirección General de Obras Públicas* (Directorate-General of Public Works)**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:***Subsecretaría de Relaciones Económicas Internacionales - Ministerio de Relaciones Exteriores de Chile* (Under-Secretariat for International Economic Relations, Ministry of Foreign Affairs of Chile) |
| **3.** | **Notified under Article 2.9.2 [X], 2.10.1 [ ], 5.6.2 [ ], 5.7.1 [ ], 3.2 [ ], 7.2 [ ], other:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Cement - Determination of fineness through wet sieving |
| **5.** | **Title, number of pages and language(s) of the notified document:** *NCh 150:2019 Cemento- Determinación de la finura por tamizado húmedo* (NCh 150:2019 Cement - Determination of fineness through wet sieving); (10 pages, in Spanish) |
| **6.** | **Description of content:** The notified rule establishes a procedure for determining the fineness of cement through wet sieving using a 0.045 mm sieve. This rule applies to cements used in the creation of mortars and concretes. This rule does not concern safety issues, if there are any, associated with its use. It is the responsibility of the user of this rule to establish appropriate health and safety practices, and to determine the degree of application of the regulatory limitations prior to use. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Quality requirements |
| **8.** | **Relevant documents:*** *NCh 162 Cemento- Extracción de muestras*
* ASTM C430 Standard Test Method for Fineness of Hydraulic Cement by the 45-um (No. 325) Sieve
* *Manual de Carreteras del MOP*, available at: <https://mc.mop.gob.cl/>
 |
| **9.** | **Proposed date of adoption:** -**Proposed date of entry into force:** - |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [ ] or address, telephone and fax numbers and email and website addresses, if available, of other body:**Subsecretaría de Relaciones Económicas InternacionalesMinisterio de Relaciones Exteriores de ChileTeatinos 180, piso 11Tel.: (+56)-2-22827 5250Email: tbt\_chile@subrei.gob.clTo view the above-mentioned standards, go to <https://www.inncoleccion.cl/> and enter the following details:*Empresa* (Company): SUBREI-003-23*Usuario* (Username): subrei*Contraseña* (Password): subrei |