NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** China  **If applicable, name of local government involved (Article 3.2 and 7.2):** |
| **2.** | **Agency responsible:** State Administration for Market Regulation (Standardization Administration of the P.R.C.)  **Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:** |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****],** **5.7.1 [****],** **other****:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Vehicles; (HS: 87 ); (ICS: 43.020) |
| **5.** | **Title, number of pages and language(s) of the notified document:** National Standard of the P.R.C., The Protection of Vehicle for Pedestrians in the Event of a Collision (43 page(s), in Chinese) |
| **6.** | **Description of content:** This  document specifies the technical requirements, test requirements, test procedures and certification of the impactor for the protection of vehicle for pedestrians in the event of a collision.  This document applies to vehicles of category M1 and N1, but it does not include category M1 no less than 2,500 kg maximum mass whose R point of driver's seat precedes the transverse plane of the front axis center or whose distance between the R point of driver's seat and the transverse plane of the front axis center is no more than 1,100 mm, and category N1 vehicles whose R point of driver's seat precedes the transverse plane of the front axis center or whose distance between the R point of driver's seat and the transverse plane of the front axis center is no more than 1,100 mm. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Management of traffic; Protection of human health or safety. |
| **8.** | **Relevant documents:** |
| **9.** | **Proposed date of adoption:** To be determined.  **Proposed date of entry into force:** For new models applying for type approval, it will be implemented after 6 months of the implementation date of this document; For models that have obtained type approval, it will be implemented after 31 months of the implementation date of this document; |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:**  WTO/TBT National Notification and Enquiry Center of the People's Republic of China Tel：+86 10 57954633/ 57954627 Email: [tbt@customs.gov.cn](mailto:tbt@customs.gov.cn)  <https://members.wto.org/crnattachments/2022/TBT/CHN/22_0473_00_x.pdf> |