NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** CHINA  **If applicable, name of local government involved (Article 3.2 and 7.2):** |
| **2.** | **Agency responsible:** State Administration for Market Regulation (Standardization Administration of the P.R.C.)  **Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:** |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****],** **5.7.1 [****], 3.2 [****], 7.2 [****],** **other****:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Vehicles (HS code(s): 87); (ICS code(s): 43.040.60) |
| **5.** | **Title, number of pages and language(s) of the notified document:** National Standard of the P.R.C., Restraining Devices for Child Occupants of Power-driven Vehicles; (121 page(s), in Chinese) |
| **6.** | **Description of content:** This document specifies the terms and definitions , general requirements, performance requirements and test methods, test reports, identification and instructions of child restraint systems for child occupants of power-driven vehicles.  This document applies to the following types of child passenger restraint systems installed on motor vehicles:  a）integral universal ISOFIX child restraint system (i-Size);  b）integral specific vehicle ISOFIX child restraint system;  c）integral universal belted child restraint system;  d）integral specific vehicle belted child restraint system;  e）non-integral universal child restraint system with backrest (i-Size booster seat);  f）non-integral specific vehicle child restraint system with backrest (specific vehicle booster seat);  g）non-integral universal child restraint system without backrest (universal booster cushion) ;  h) non-integral specific vehicle child restraint system without backrest (specific vehicle booster cushion). |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Protection of human health or safety; Quality requirements |
| **8.** | **Relevant documents:** - |
| **9.** | **Proposed date of adoption:** To be determined  **Proposed date of entry into force:** 12 months after approval |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:**  WTO/TBT National Notification and Enquiry Center of the People's Republic of China  Tel：+86 10 57954633/ 57954627  E\_mail: [tbt@customs.gov.cn](mailto:tbt@customs.gov.cn)  <https://members.wto.org/crnattachments/2022/TBT/CHN/22_5742_00_x.pdf> |