NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Jamaica  **If applicable, name of local government involved (Article 3.2 and 7.2):** |
| **2.** | **Agency responsible:** Bureau of Standards Jamaica  **Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:**  Regional and International Trade Branch 6 Winchester Road Kingston 10 Jamaica W.I. Email: [tbtenquirypoint@bsj.org.jm](mailto:tbtenquirypoint@bsj.org.jm); Website: <http://www.bsj.org.jm> Tel.: 1 (876) 926-3140-5/ (876) 618-1534/ (876) 632-4275; Fax: 1 (876) 929-4736 |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****],** **5.7.1 [****],** **other****:** |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Vessels and containers mounted on vehicles (ICS 23.020.20) |
| **5.** | **Title, number of pages and language(s) of the notified document:** Standard Specification for The Repair and Rebuilding of Low-pressure Welded Steel Transportable Gas Containers. (21 page(s), in English) |
| **6.** | **Description of content:** This Jamaican Standard specifies requirements for the repair and rebuilding of low-pressure transportable gas containers and the subsequent testing of these transportable gas containers before re-use. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** This standard specifies the requirements for the repair and rebuilding of low-pressure transportable gas containers made in accordance with JS 25 Jamaican Standard Specification for Transportable gas containers, and the subsequent testing of these transportable gas containers before re-use. This standard does not apply to containers designed and manufactured to contain dissolved acetylene. Repairs to valves and fittings, which are not permanent attachments to the transportable gas container, shall not be covered by this standard.  The revised standard is intended to be mandatory and aims to provide assurance that adequate health and safety protection exists for the intended users of the cylinders.; Protection of human health or safety |
| **8.** | **Relevant documents:**  A notice of the *Standard Speciﬁcation for The Repair and Rebuilding of Low-pressure Welded Steel Transportable Gas* will appear in The Jamaica Gazette Supplement - Proclamations, Rules and Regulations. The document will appear as a Jamaican Standard Specification, with mandatory status, and will be available for sale. |
| **9.** | **Proposed date of adoption:** 21 November 2022  **Proposed date of entry into force:** 21 November 2022 |
| **10.** | **Final date for comments:** 21 February 2022 |
| **11.** | **Texts available from: National enquiry point [** **]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:**  Bureau of Standards Jamaica (BSJ) Regional & International Trade Branch 6 Winchester Road  Kingston 10  +(876)-618-1534; +(876)-632-4275 [tbtenquirypoint@bsj.org.jm](mailto:tbtenquirypoint@bsj.org.jm)  <http://www.bsj.org.jm>  info@bsj.org.jm |