NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Tanzania **If applicable, name of local government involved (Article 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** Tanzania Bureau of Standards (TBS); MOROGORO/Sam Nujoma Road, Ubungo ;P O BOX 9524, Dar es Salaam, Tanzania;Tel: +255 222450206;E- mail: nep@tbs.go.tz;Website: [www.tbs.go.tz.](http://www.tbs.go.tz.)**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:**  |
| **3.** | **Notified under Article 2.9.2 [****X],** **2.10.1 [****],** **5.6.2 [****],** **5.7.1 [****],** **other****:**  |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Articles of iron or steel wire, n.e.s (HS 732620); Other construction materials (ICS 91.100.99) |
| **5.** | **Title, number of pages and language(s) of the notified document:** MEDC 02 (1037),Metal roofing tiles — Specification, Third Edition (12 page(s), in English) |
| **6.** | **Description of content:** This specification covers requirements for metal roofing tiles (coated or uncoated) supplied in the form of carbon steel sheets or aluminium alloy sheets (each comprising a series of simulated tile units) and for trim sections (of the same materials) designed for use in conjunction with tile units of the same material and of appropriate profile |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Consumer information, labelling; Quality requirements; Reducing trade barriers and facilitating trade |
| **8.** | **Relevant documents:** ASTM G 153, Standard practice for operating enclosed carbon arc light apparatus for exposure of non-metallic materials.SANS 903, Aluminium alloy corrugated and troughed sheets.ISO 3575, Continuous hot-dip zinc-coated carbon steel sheet of commercial and drawing qualities.ISO 4998, Continuous hot-dip zinc-coated carbon steel sheet of structural quality.SANS 5146, Paints and varnishes – Resistance to impact of paint filmsISO 7253, Paints and varnishes – Determination of resistance to neutral salt spray (fog).ISO 9227, Corrosion tests in artificial atmospheres – Salt spray tests.ISO 9364, Continuous hot-dip aluminium/zinc-coated steel sheet of commercial, drawing and structural qualities.SABS 1022:2013, published by the South African Bureau of Standards Metal roofing tiles — Specification.SANS 5146:2005, Paints and vanishes — Resistance to impact of paint film, published by the South African Bureau of Standards |
| **9.** | **Proposed date of adoption:** To be determined**Proposed date of entry into force:** To be determined |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:** Contact person(s):Ms. Bahati Samillani (NEP officer) and Mr. Clavery ChausiTanzania Bureau of Standards (TBS)Morogoro/Sam Nujoma Road, UbungoP O Box 9524Dar Es Salaam+(255) 22 2450206nep@tbs.go.tz; bahati.samillani@tbs.go.tz<http://www.tbs.go.tz><https://members.wto.org/crnattachments/2022/TBT/TZA/22_0189_00_e.pdf> |