NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** Uganda **If applicable, name of local government involved (Article 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** Uganda National Bureau of StandardsPlot 2-12 ByPass Link, Bweyogerere Industrial and Business ParkP.O. Box 6329Kampala, UgandaTel: +(256) 4 1733 3250/1/2Fax: +(256) 4 1428 6123E-mail: info@unbs.go.ugWebsite: <https://www.unbs.go.ug>**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:**  |
| **3.** | **Notified under Article 2.9.2 [****],** **2.10.1 [****],** **5.6.2 [****X],** **5.7.1 [****],** **other****:**  |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Engine Coolant; Anti-freezing preparations and prepared de-icing fluids (excl. prepared additives for mineral oils or other liquids used for the same purposes as mineral oils) (HS 3820); Refrigerants and antifreezes (ICS 71.100.45) |
| **5.** | **Title, number of pages and language(s) of the notified document:** DUS 2405:2021, Standard Test Method for Determination of Silicon and Other Elements in Engine Coolant by Inductively Coupled Plasma-Atomic Emission Spectroscopy, First Edition (12 page(s), in English) |
| **6.** | **Description of content:** This Draft Uganda Standard covers the determination of silicon in engine coolant by inductively coupled plasma-atomic emission spectroscopy (ICP-AES). Silicon can be determined as low as the range of 5 ppm by this test method. Other elements also found in engine coolant can be determined by this method. This test method is applicable to the determination of dissolved or dispersed elements. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Prevention of deceptive practices and consumer protection; Quality requirements |
| **8.** | **Relevant documents:** 1. ASTM D1176 Practice for Sampling and Preparing Aqueous Solutions of Engine Coolants or Antirusts for Testing Purposes
2. ASTM D1193 Specification for Reagent Water
3. ASTM E177 Practice for Use of the Terms Precision and Bias in ASTM Test Methods
4. ASTM E691 Practice for Conducting an Interlaboratory Study to Determine the Precision of a Test Method
5. Method 6010, Inductively Coupled Plasma Method, SW-846, Test Methods for Evaluating Solid Waste
6. Method 200.7, Inductively Coupled Plasma - Atomic Emission Spectrometric Method for Trace Element Analysis of Water And Wastes, EPA-600/4-79-020, revised 1984
 |
| **9.** | **Proposed date of adoption:** December 2021**Proposed date of entry into force:** Not applicable |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:** Uganda National Bureau of StandardsPlot 2-12 ByPass Link, Bweyogerere Industrial and Business ParkP.O. Box 6329Kampala, UgandaTel: +(256) 4 1733 3250/1/2Fax: +(256) 4 1428 6123E-mail: info@unbs.go.ugWebsite: <https://www.unbs.go.ug> |