NOTIFICATION

The following notification is being circulated in accordance with Article 10.6

|  |  |
| --- | --- |
| **1.** | **Notifying Member:** UGANDA**If applicable, name of local government involved (Article 3.2 and 7.2):**  |
| **2.** | **Agency responsible:** Uganda National Bureau of StandardsPlot 2-12 ByPass Link, Bweyogerere Industrial and Business ParkP.O. Box 6329Kampala, UgandaTel: +(256) 4 1733 3250/1/2Fax: +(256) 4 1428 6123E-mail: info@unbs.go.ugWebsite: <https://www.unbs.go.ug>**Name and address (including telephone and fax numbers, email and website addresses, if available) of agency or authority designated to handle comments regarding the notification shall be indicated if different from above:**  |
| **3.** | **Notified under Article 2.9.2 [****],** **2.10.1 [****],** **5.6.2 [****X],** **5.7.1 [****], 3.2 [****], 7.2 [****],** **other****:**  |
| **4.** | **Products covered (HS or CCCN where applicable, otherwise national tariff heading. ICS numbers may be provided in addition, where applicable):** Petroleum gases and other gaseous hydrocarbons. (HS code(s): 2711); Fuels (ICS code(s): 75.160) |
| **5.** | **Title, number of pages and language(s) of the notified document:** **DUS 2525:2022, Standard Test Method for Gravimetric Measurement of Particulate Concentration of Hydrogen Fuel, First edition**; (10 page(s), in English) |
| **6.** | **Description of content:** This Draft Uganda Standard is primarily intended for gravimetric determination of particulate concentration in hydrogen intended as a fuel for fuel cell or internal combustion engine powered vehicles. This test method describes operating and quality control procedures required to obtain data of known quality satisfying the requirements of SAE J2719. This test method can be applied to other gaseous samples requiring determination of particulates provided the user's data quality objectives are satisfied. |
| **7.** | **Objective and rationale, including the nature of urgent problems where applicable:** Prevention of deceptive practices and consumer protection; Quality requirements |
| **8.** | **Relevant documents:** 1. ASTM D4150
2. ASTM D7650
3. ASTM E617
4. SAE J2600 Compressed Hydrogen Surface Vehicle Refueling Connection Devices
5. SAE J2719 Hydrogen Quality Guideline for Fuel Cell Vehicles
6. Code of Federal Regulations, Title 40, Part 50, Appendix L, Section 8.24
7. ISO 14687–2 Hydrogen fuel -- Product specification -- Part 2: Proton exchange membrane (PEM) fuel cell applications for road vehicles
 |
| **9.** | **Proposed date of adoption:** To be determined**Proposed date of entry into force:** Not applicable. |
| **10.** | **Final date for comments:** 60 days from notification |
| **11.** | **Texts available from: National enquiry point [****X]** **or address, telephone and fax numbers and email and website addresses, if available, of other body:** Uganda National Bureau of StandardsPlot 2-12 ByPass Link, Bweyogerere Industrial and Business ParkP.O. Box 6329Kampala, UgandaTel: +(256) 4 1733 3250/1/2Fax: +(256) 4 1428 6123E-mail: info@unbs.go.ugWebsite: <https://www.unbs.go.ug> |